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Views of the Iwan
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Mirror on façade

	
HYBRID houses :
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Assessment of 
The level 
Of natural lighting
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 Movable walls of glass and wood animate

	
NEO MOORISH houses :
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Mobile sliding roof canopy


	NEO CLASSICAL
buildings : 
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Views of the exterior facade 
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Shelf reflectors, are reflective awnings over the windows
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ART DECO buildings :
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view of the Court
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openings with adjustable blades













	In the extramural context

	House type
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	Adaptive interpretation

	
ART DECO buildings :
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High windows in the patio
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Light shelves




	MOORISH houses :
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Horizontal windows

	INTEGRATED HOUSES type large sets:
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Glazed railing


	Service buildings

	MOSQUE :
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contemporary mosque cover

	SCHOOL : 
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Glazed panel protected by moucharabiehs

	HAMMAM : 
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Skylights



Table 2: The hierarchical set of models [Author, 2023]
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